README FOR:  Textures in SRVRusty.zip and the archived contents.

WARNING!!! Although I am generally using a route standard naming for .ace .s and .sd file. I am Not responsable if you accidently overwrite an existing .ace, .s, or .sd file and screw up your route. If in doubt, back up your textures and shapes file before installing. Other shapes using the SRV_ prefix from my submissions may share the same ace textures and will not be affected if they are overwritten.

Contents: Three common bridge kit textures shared by many present and future bridge kit textured in rusty and other submissions. Textures are being submitted separately so that future file downloads that share them will be smaller.

to install:
1: unzip to a temp folder with "use folder names" on.

2: Copy the Three textures from the texture folder to the texture folder of your route you are using them in. Replace your existing SRV_Bridges2.ace only if you have a bridge that displays white in the lattace girders.

3: Optionally, copy the Three textures from TSModelerTextures and place them where TSmodeler or your favorite 3-d modeling program can find them.


	The contents of SRVRusty.zip can be used by MSTS route designers so long as those routes are distributed without charge.
	Please notify me for additional permission if you plan to distribute your route or the content by CD. You may use such content as long as your charge is to recover the cost of the media and shipping to the intended user.

Ron Picardi,
rpicardi1@chartermi.net